{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":17,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH12E / EPRA08-12EW"]
[]
[]
[]
[]
["","","","","","ETSH12P30EF / EPRA08EAW1","ETSH12P50EF / EPRA08EAW1","ETSH12P30EG / EPRA08EAW1","ETSH12P50EG / EPRA08EAW1","ETSH12P30EF / EPRA10EAW1","ETSH12P50EF / EPRA10EAW1","ETSH12P30EG / EPRA10EAW1","ETSH12P50EG / EPRA10EAW1","ETSH12P30EF / EPRA12EAW1","ETSH12P50EF / EPRA12EAW1","ETSH12P30EG / EPRA12EAW1","ETSH12P50EG / EPRA12EAW1"]
["Notranja enota","","","","","ETSH12P30EF","ETSH12P50EF","ETSH12P30EG","ETSH12P50EG","ETSH12P30EF","ETSH12P50EF","ETSH12P30EG","ETSH12P50EG","ETSH12P30EF","ETSH12P50EF","ETSH12P30EG","ETSH12P50EG"]
["Grelna kapaciteta","Nom.","","","kW","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)"]
["Vhodna moč","Gretje","","Nom.","kW","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)"]
["COP","","","","","5.1","5.1","5.10 (1)","5.10 (1)","5.1","5.1","5.10 (1)","5.10 (1)","5.1","5.1","5.10 (1)","5.10 (1)"]
["Gretje sanitarne tople vode","Splošno","","Profil deklarirane obremenitve","","L","XL","L","XL","L","XL","L","XL","L","XL","L","XL"]
["","Povprečno podnebje","","Razred energijske učinkovitosti gretje vode","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Ogrevanje prostora","Izhod vode v povprečnem podnebju 55°C","Splošno","SCOP","","3.52","3.52","3.52","3.52","3.53","3.53","3.53","3.53","3.53","3.53","3.53","3.53"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Izhod vode v povprečnem podnebju 35°C","Splošno","SCOP","","4.81","4.81","4.81","4.81","4.84","4.84","4.84","4.84","4.84","4.84","4.84","4.84"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Razpon energetske učinkovitosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Opombe","","","","","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(2) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti"]