{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB-D / EPRA014-018DV"]
[]
[]
[]
[]
["","","","","","ETSHB16P30DA / EPRA14DAV3","ETSHB16P50DA / EPRA14DAV3","ETSHB16P30DA / EPRA16DAV3","ETSHB16P50DA / EPRA16DAV3","ETSHB16P30DA / EPRA18DAV3","ETSHB16P50DA / EPRA18DAV3"]
["Notranja enota","","","","","ETSHB16P30DA","ETSHB16P50DA","ETSHB16P30DA","ETSHB16P50DA","ETSHB16P30DA","ETSHB16P50DA"]
["Grelna kapaciteta","Min.","","","kW","3.70","3.70","3.96","3.96","4.40","4.40"]
["","Nom.","","","kW","5.69","5.69","9.00","9.00","9.00","9.00"]
["","Maks.","","","kW","10.18","10.18","10.91","10.91","12.12","12.12"]
["Vhodna moč","Gretje","","Min.","kW","0.88","0.88","0.95","0.95","1.05","1.05"]
["","","","Nom.","kW","1.22","1.22","1.80","1.80","1.80","1.80"]
["","","","Maks.","kW","2.09","2.09","2.24","2.24","2.49","2.49"]
["","Segrevanje gospodinjske vode od 10°C do 50°C","","Naz.","kWh","3.92","5.26","3.92","5.26","3.92","5.26"]
["Čas segrevanja od 10°C do 50°C","ure","","","","9ur 20 min pri zunanji temperaturi 7°C","2 uri 11 min. pri zunanji temperaturi 7 °C","9ur 20 min pri zunanji temperaturi 7°C","2 uri 11 min. pri zunanji temperaturi 7 °C","9ur 20 min pri zunanji temperaturi 7°C","2 uri 11 min. pri zunanji temperaturi 7 °C"]
["COP","","","","","4.67","4.67","5.00","5.00","5.00","5.00"]
["Gretje sanitarne tople vode","Splošno","","Profil deklarirane obremenitve","","L","XL","L","XL","L","XL"]
["","Povprečno podnebje","","Razred energijske učinkovitosti gretje vode","","A","A","A","A","A","A"]
["Ogrevanje prostora","Izhod vode v povprečnem podnebju 55°C","Splošno","SCOP","","3.58","3.58","3.58","3.58","3.58","3.58"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A++","A++","A++","A++","A++","A++"]
["","Izhod vode v povprečnem podnebju 35°C","Splošno","SCOP","","4.51","4.51","4.51","4.51","4.51","4.51"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Opombe","","","","","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C"]
["","","","","","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)"]
["","","","","","(3) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(3) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(3) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(3) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(3) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(3) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511"]
["Razpon energetske učinkovitosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F","","Space Heating A+++ ~ D, Water Heating A+ ~ F"]