{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":17,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB12E / EPRA08-12EV"]
[]
[]
[]
[]
["","","","","","ETSHB12P30EF / EPRA08EAV3","ETSHB12P50EF / EPRA08EAV3","ETSHB12P30EG / EPRA08EAV3","ETSHB12P50EG / EPRA08EAV3","ETSHB12P30EF / EPRA10EAV3","ETSHB12P50EF / EPRA10EAV3","ETSHB12P50EG / EPRA10EAV3","ETSHB12P30EG / EPRA10EAV3","ETSHB12P30EF / EPRA12EAV3","ETSHB12P50EF / EPRA12EAV3","ETSHB12P30EG / EPRA12EAV3","ETSHB12P50EG / EPRA12EAV3"]
["Notranja enota","","","","","ETSHB12P30EF","ETSHB12P50EF","ETSHB12P30EG","ETSHB12P50EG","ETSHB12P30EF","ETSHB12P50EF","ETSHB12P50EG","ETSHB12P30EG","ETSHB12P30EF","ETSHB12P50EF","ETSHB12P30EG","ETSHB12P50EG"]
["Grelna kapaciteta","Nom.","","","kW","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)"]
["Vhodna moč","Gretje","","Nom.","kW","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)","1.25 (1)"]
["COP","","","","","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)","4.92 (3)"]
["Gretje sanitarne tople vode","Splošno","","Profil deklarirane obremenitve","","L","XL","L","XL","L","XL","XL","L","L","XL","L","XL"]
["","Povprečno podnebje","","Razred energijske učinkovitosti gretje vode","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Ogrevanje prostora","Izhod vode v povprečnem podnebju 55°C","Splošno","SCOP","","3.41","3.41","3.41","3.41","3.43","3.43","3.43","3.43","3.43","3.43","3.43","3.43"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Izhod vode v povprečnem podnebju 35°C","Splošno","SCOP","","4.69","4.69","4.69","4.69","4.71","4.71","4.71","4.71","4.71","4.71","4.71","4.71"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Razpon energetske učinkovitosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Opombe","","","","","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. pogoj: hlajenje Ta 35 °C - LWE 18 °C (DT = 5 °C); ogrevanje Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)"]
["","","","","","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti","(3) - DB/WB 7 °C/6 °C - LWC 35 °C (dT=5 °C) s črpalko na polni hitrosti"]