{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB16E / EPRA14-18DV7"]
[]
[]
[]
[]
["","","","","","ETSHB16P30EF / EPRA14DAV37","ETSHB16P50EF / EPRA14DAV37","ETSHB16P30EF / EPRA16DAV37","ETSHB16P50EF / EPRA16DAV37","ETSHB16P30EF / EPRA18DAV37","ETSHB16P50EF / EPRA18DAV37"]
["Grelna kapaciteta","Min.","","","kW","37.00 (1)","37.00 (1)","396.00 (1)","396.00 (1)","44.00 (1)","44.00 (1)"]
["","Nom.","","","kW","569 (2)","569 (2)","9.00 (2)","9.00 (2)","9.00 (2)","9.00 (2)"]
["","Maks.","","","kW","1,018.00 (1)","1,018.00 (1)","1,091.00 (1)","1,091.00 (1)","1,212.00 (1)","1,212.00 (1)"]
["Vhodna moč","Gretje","","Min.","kW","88.00 (5)","88.00 (5)","95.00 (5)","95.00 (5)","105.00 (5)","105.00 (5)"]
["","","","Nom.","kW","122 (2)","122 (2)","18.0 (2)","18.0 (2)","18.0 (2)","18.0 (2)"]
["","","","Maks.","kW","209.00 (5)","209.00 (5)","224.00 (5)","224.00 (5)","249.00 (5)","249.00 (5)"]
["COP","","","","","467.00 (2)","467.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)","5.00 (2)"]
["Gretje sanitarne tople vode","Splošno","","Profil deklarirane obremenitve","","L","XL","L","XL","L","XL"]
["","Povprečno podnebje","","Razred energijske učinkovitosti gretje vode","","A+","A+","A+","A+","A+","A+"]
["Ogrevanje prostora","Izhod vode v povprečnem podnebju 55°C","Splošno","SCOP","","3.58","3.58","3.58","3.58","3.58","3.58"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A++","A++","A++","A++","A++","A++"]
["","Izhod vode v povprečnem podnebju 35°C","Splošno","SCOP","","4.51","4.51","4.51","4.51","4.51","4.51"]
["","","","Razred učinkovitosti sezonskega ogrevanja prostora","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Razpon energetske učinkovitosti","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Opombe","","","","","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C","(1) - Zmogljivost v skladu s standardom EN14511 in veljavna za toplo vodo v razponu dT = 3~8 °C pri Ta 7 °C"]
["","","","","","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(2) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)"]
["","","","","","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(3) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB"]
["","","","","","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(4) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB"]
["","","","","","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511","(5) - Vhodna moč je skupna vhodna moč notranjih in zunanjih enot, vključno z obtočno črpalko; v skladu z EN14511"]