{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB16E"]
[]
[]
[]
[]
["","","","","","ETSHB16P30EF","ETSHB16P50EF"]
["Ohišje","Colour","","","","Bela (RAL9016) / Črna (RAL9017)","Bela (RAL9016) / Črna (RAL9017)"]
["","Material","","","","Na udarec odporen polipropilen","Na udarec odporen polipropilen"]
["Mere","Enota","","Višina","mm","1,892","1,910"]
["","","","Širina","mm","594","792"]
["","","","Globina","mm","644","816"]
["Teža","Enota","","","kg","76","100"]
["Sound power level","Nom.","","","dBA","45.6","45.6"]
["Raven zvočnega tlaka","Nom.","","","dBA","32.8","32.8"]
["Območje delovanja","Ogrevanje","Stran vode","Min.","°C","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)"]
["","Hlajenje","Okolje","Min.","°CDB","0 (2)","0 (2)"]
["","","Stran vode","Min.","°C","0 (2)","0 (2)"]
["","","","Maks.","°C","0 (2)","0 (2)"]
["Power supply","Phase","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","230","230"]
["Opombe","","","","","(1) - Toplotna izguba v skladu z EN12897","(1) - Toplotna izguba v skladu z EN12897"]
["","","","","","(2) - Glejte diagrame obratovalnih omejitev","(2) - Glejte diagrame obratovalnih omejitev"]