{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSX-D"]
[]
[]
[]
[]
["","","","","","ETSX16P30DA","ETSX16P50DA"]
["Raven zvočnega tlaka","Nom.","","","dBA","32.8","32.8"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","10","10"]
["","","Stran vode","Maks.","°C","22","22"]
["","","","Min.","°C","5","5"]
["","Ogrevanje","Stran vode","Maks.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Sound power level","Nom.","","","dBA","45.6","45.6"]
["Mere","Enota","","Širina","mm","590","785"]
["","","","Globina","mm","615","785"]
["","","","Višina","mm","1,891","1,896"]
["Ohišje","Material","","","","Na udarec odporen polipropilen","Na udarec odporen polipropilen"]
["","Colour","","","","Bela (RAL9016) / Temno siva (RAL7011)","Bela (RAL9016) / Temno siva (RAL7011)"]
["PED","Category","","","","Čl. 4.3","Čl. 4.3"]
["Teža","Enota","","","kg","73","90"]
["Power supply","Phase","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","230","230"]
["Električni grelnik","Napajanje","","Frekvenca","Hz","50","50"]
["","","","Ime","","3V / 9W","3V / 9W"]
["","","","Faza","","1~ / 3~","1~ / 3~"]
["Opombe","","","","","(1) - Toplotna izguba v skladu z EN12897","(1) - Toplotna izguba v skladu z EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C","(3) - TKW = 10°C/TWW = 40°C/TSP = 60°C"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]