{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":9,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYA-DW1P-H-"]
[]
[]
[]
[]
["","","","","","EWYA009DAW1P-H-","EWYA011DAW1P-H-","EWYA014DAW1P-H-","EWYA016DAW1P-H-"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","44.0","47.7","50.8","51.0"]
["Hidravlične komponente","Ekspanzijska posoda","","Prostornina","l","8","8","8","8"]
["Delovni doseg","Stran zraka","Hlajenje","Min.","°CDB","10","10","10","10"]
["","","","Maks.","°CDB","43","43","43","43"]
["","","Gretje","Maks.","°CDB","25","25","25","25"]
["","","","Min.","°CDB","-25","-25","-25","-25"]
["","Stran vode","Gretje","Min.","°CDB","9 (7)","9 (7)","9 (7)","9 (7)"]
["","","","Maks.","°CDB","60 (7)","60 (7)","60 (7)","60 (7)"]
["","","Hlajenje","Maks.","°CDB","22","22","22","22"]
["","","","Min.","°CDB","5","5","5","5"]
["Polnitev hladilnega sredstva","Na krogotok","","","kg","3.80","3.80","3.80","3.80"]
["","Refrigerant charge-=-Per circuit-=-TCO2Eq","","","TCO2Eq","2.6","2.6","2.6","2.6"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni inverterski kompresor","Hermetično zaprt nihajni inverterski kompresor","Hermetično zaprt nihajni inverterski kompresor","Hermetično zaprt nihajni inverterski kompresor"]
["","Način zagona_","","","","Invertersko gnan","Invertersko gnan","Invertersko gnan","Invertersko gnan"]
["","Količina","","","","1","1","1","1"]
["Zračni toplotni izmenjevalnik","Tip","","","","Visoko učinkovito tip rebra in cevi z integralnim podhladilnikom","Visoko učinkovito tip rebra in cevi z integralnim podhladilnikom","Visoko učinkovito tip rebra in cevi z integralnim podhladilnikom","Visoko učinkovito tip rebra in cevi z integralnim podhladilnikom"]
["Teža","Enota","","","kg","147","147","147","147"]
["EER","","","","","3.35 (1), 5.34 (2)","3.26 (1), 5.31 (2)","3.16 (1), 5.04 (2)","3.06 (1), 4.74 (2)"]
["Hladilno sredstvo","GWP","","","","675.0","675.0","675.0","675.0"]
["","Tip","","","","R-32","R-32","R-32","R-32"]
["","Vezja","","Količina","","1","1","1","1"]
["","Krmiljenje","","","","Elektronski ekspanzijski ventil","Elektronski ekspanzijski ventil","Elektronski ekspanzijski ventil","Elektronski ekspanzijski ventil"]
["Motor ventil.","Hitrost","Hlajenje","Nom.","vrt/min","500","550","650","650"]
["","","Gretje","Nom.","vrt/min","400","450","550","650"]
["Hladilna kapaciteta","Nom.","","","kW","9.35 (1), 9.10 (2)","11.6 (1), 11.5 (2)","12.8 (1), 12.7 (2)","14.0 (1), 15.3 (2)"]
["Vodni toplotni izmenjevalnik","Volumen vode","","","l","2","2","2","2"]
["","Minimalni volumen vode v sistemu","","","l","50 (6)","50 (6)","50 (6)","50 (6)"]
["","Tip","","","","Ploščni toplotni izmenjevalnik","Ploščni toplotni izmenjevalnik","Ploščni toplotni izmenjevalnik","Ploščni toplotni izmenjevalnik"]
["Vhodna moč","Hlajenje","","Nom.","kW","2.79 (1), 1.71 (2)","3.56 (1), 2.17 (2)","4.06 (1), 2.51 (2)","4.58 (1), 3.24 (2)"]
["","Gretje","","Nom.","kW","1.91 (3), 2.43 (4)","2.18 (3), 2.68 (4)","2.46 (3), 3.42 (4)","3.53 (3), 4.56 (4)"]
["Sound power level","Hlajenje","","Nom.","dBA","65.5","67.0","69.0","69.0"]
["COP","","","","","4.91 (3), 3.71 (4)","4.83 (3), 3.66 (4)","4.87 (3), 3.64 (4)","4.53 (3), 3.51 (4)"]
["Mere","Enota","","Širina","mm","1,380","1,380","1,380","1,380"]
["","","","Globina","mm","460","460","460","460"]
["","","","Višina","mm","870","870","870","870"]
["Krmiljenje kapacitete","Metoda","","","","Spremenljivo (inverter)","Spremenljivo (inverter)","Spremenljivo (inverter)","Spremenljivo (inverter)"]
["Ogrevanje prostora","Izhod vode v povprečnem podnebju 55°C","Splošno","Seasonal space heating eff. class","","A++","A++","A++","A++"]
["","","","ηs (Sezonska učinkovitost ogrevanja prostora)","%","135","132","134","132"]
["","","","SCOP","","3.44","3.37","3.42","3.37"]
["Ventilator","Hitrost pretoka zraka","Gretje","Nom.","m³/min","48.0","55.8","70.4","85.0"]
["","","Hlajenje","Nom.","m³/min","63","70","85","85"]
["Grelna kapaciteta","Nom.","","","kW","9.37 (3), 9.00 (4)","10.6 (3), 9.82 (4)","12.0 (3), 12.5 (4)","16.0 (3), 16.0 (4)"]
["Kompresor","Način zagona_","","","","Inverter","Inverter","Inverter","Inverter"]
["Power supply","Faza","","","","3~","3~","3~","3~"]
["","Frekvenca","","","Hz","50","50","50","50"]
["","Ime","","","","W1","W1","W1","W1"]
["","Napetost","","","V","400","400","400","400"]
["Opombe","","","","","(1) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(1) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(1) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB","(1) - Hlajenje: EW 12°C; LW 7°C; okoljski pogoji: 35°CDB"]
["","","","","","(2) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(2) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(2) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB","(2) - Hlajenje: EW 23°C; LW 18°C; okoljski pogoji: 35°CDB"]
["","","","","","(3) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(3) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(3) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)","(3) - Pogoji: Ta DB/WB 7° C/6° C - LWC 35° C (DT = 5° C)"]
["","","","","","(4) - Pogoji: Ta DB/WB 7° C/6° C - LWC 45° C (Dt=5° C)","(4) - Pogoji: Ta DB/WB 7° C/6° C - LWC 45° C (Dt=5° C)","(4) - Pogoji: Ta DB/WB 7° C/6° C - LWC 45° C (Dt=5° C)","(4) - Pogoji: Ta DB/WB 7° C/6° C - LWC 45° C (Dt=5° C)"]
["","","","","","(5) - V skladu z EN14825","(5) - V skladu z EN14825","(5) - V skladu z EN14825","(5) - V skladu z EN14825"]
["","","","","","(6) - Odvisno od tipa obratovalnega načina, glejte priročnik za namestitev.","(6) - Odvisno od tipa obratovalnega načina, glejte priročnik za namestitev.","(6) - Odvisno od tipa obratovalnega načina, glejte priročnik za namestitev.","(6) - Odvisno od tipa obratovalnega načina, glejte priročnik za namestitev."]
["","","","","","(7) - Več podrobnosti preverite na risbi z obratovalnim razponom","(7) - Več podrobnosti preverite na risbi z obratovalnim razponom","(7) - Več podrobnosti preverite na risbi z obratovalnim razponom","(7) - Več podrobnosti preverite na risbi z obratovalnim razponom"]