{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":9,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EWYT-CZI"]
[]
[]
[]
[]
["","","","","","EWYT021CZI-A1","EWYT032CZI-A1","EWYT040CZI-A1","EWYT064CZI-A2"]
["Ohišje","Barva","","","","Slonovinasto bela","Slonovinasto bela","Slonovinasto bela","Slonovinasto bela"]
["","Material","","","","Galvanizirana in pobarvana jeklena pločevina","Galvanizirana in pobarvana jeklena pločevina","Galvanizirana in pobarvana jeklena pločevina","Galvanizirana in pobarvana jeklena pločevina"]
["Mere","Enota","","Višina","mm","700","700","700","700"]
["","","","Širina","mm","1,120","1,120","1,120","1,120"]
["","","","Globina","mm","830","830","830","830"]
["Teža","Enota","","","kg","133","144","144","172"]
["Raven zvočne moči","Nom.","","","dBA","63.0","64.5","64.5","66.0"]
["Območje delovanja","Gretje","Stran vode","Min.","°C","20","20","20","20"]
["","","","Maks.","°C","60","60","60","60"]
["","Hlajenje","Okolje","Min.","°CDB","-20","-20","-20","-20"]
["","","Stran vode","Min.","°C","4","4","4","4"]
["","","","Maks.","°C","20","20","20","20"]
["Napajanje","Faza","","","","3N~","3N~","3N~","3N~"]
["","Frekvenca","","","Hz","50","50","50","50"]
["","Napetost","","","V","400","400","400","400"]