{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / FAA71BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG125L8Y1B","FAA100BUV1B / RZQG100L8Y1B","FAA71BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG71L8Y1B"]
["Hladilna kapaciteta","Nom.","","kW","","","","6.80","6.80"]
["Hlajenje prostora","SEER","","","","","","6.43","6.43"]
["","Letna poraba energije","","kWh/a","","","","371","371"]
["","Zmogljivost","Pdizajn","kW","","","","6.80","6.80"]
["","Razred energijske učinkovitosti","","","","","","A++","A++"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","","","","6.33","6.33"]
["","SCOP/A","","","","","","4.02","4.02"]
["","Razred energijske učinkovitosti","","","","","","A+","A+"]
["","Letna poraba energije","","kWh/a","","","","2,205","2,205"]
["Nazivna učinkovitost","EER","","","","","","3.40","3.40"]
["","Letna por.energ.","","kWh","","","","1,000"]
["","COP","","","","","","3.70"]
["","Direktiva o energijskih oznakah","Hlajenje","","","","","A"]
["","","Ogrevanje","","","","","A"]
["Grelna kapaciteta","Nom.","","kW","","","","7.50"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Opombe","","","","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Glejte ločeno risbo za električne podatke"]
["","","","","","","","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","","","(4) - Glejte ločeno risbo za električne podatke"]