{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Ohišje","Barva","","","","Bela","Bela"]
["","Material","","","","Smola","Smola"]
["Mere","Enota","","Višina","mm","290","340"]
["","","","Širina","mm","1050","1200"]
["","","","Globina","mm","269","262"]
["Teža","Enota","","","kg","14","18"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","16.2","23"]
["","","","Srednja","m³/min","13.4","21.1"]
["","","","Nizko","m³/min","12.1","18.7"]
["","","Gretje","Visok","m³/min","16.9","23"]
["","","Ogrevanje","Srednja","m³/min","14.2","20.9"]
["","","Gretje","Nizko","m³/min","12.7","18.7"]
["Raven zvočne moči","Hlajenje","","","dBA","61","65"]
["","Gretje","","","dBA","61","65"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","45","49"]
["","","","Srednja","dBA","42","45"]
["","","","Nizko","dBA","40","41"]
["","Gretje","","Visok","dBA","45","49"]
["","Ogrevanje","","Srednja","dBA","42","45"]
["","Gretje","","Nizko","dBA","40","41"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","9.52","9.52"]
["","Plin","","Zun. premer","mm","15.9","15.9"]
["","Izpust","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","220-240","220-240"]
["Standardni pripomočki","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Opombe","","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["Standardni pripomočki","Screw cover","","","","","3"]