{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Raven zvočnega tlaka","Gretje","Visok","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["","","Srednja","dBA","42","45"]
["","","Nizko","dBA","40","41"]
["","Hlajenje","Srednja","dBA","42","45"]
["","","Nizko","dBA","40","41"]
["","","Visok","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["Hladilna kapaciteta","Skupna kapaciteta","Nom.","kW","0.051","0.061"]
["Priključki napeljave","Tekočina","Zun. premer","mm","9.52","9.52"]
["","Plin","Zun. premer","mm","15.9","15.9"]
["","priključka","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Sound power level","Hlajenje","","dBA","61","65"]
["","Gretje","","dBA","61","65"]
["Mere","Enota","Širina","mm","1,050","1,200"]
["","","Globina","mm","238","240"]
["","","Višina","mm","290","340"]
["Ohišje","Material","","","Smola","Smola"]
["","Barva","","","Sveže bela","Sveže bela"]
["Teža","Enota","","kg","13","17"]
["Grelna kapaciteta","Skupna kapaciteta","Nom.","kW","0.068","0.061"]
["Power supply","Faza","","","1~","1~"]
["","Frekvenca","","Hz","50","50"]
["","Napetost","","V","220-240","220-240"]