{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RZQ-C"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / FBA50A2VEB9 / RZQ200C7Y1B","FBA60A2VEB9 / FBA60A2VEB9 / FBA60A2VEB9 / FBA60A2VEB9 / RZQ250C7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","20.0 (1)"]
["Hlajenje prostora","SEER","","","5.67"]
["","Letna poraba energije","","kWh/a","2,115"]
["","Zmogljivost","Pdizajn","kW","20.0"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","11.2"]
["","SCOP/A","","","3.68"]
["","Letna poraba energije","","kWh/a","4,257"]
["Grelna kapaciteta","Nom.","","kW","23.0 (2)"]
["Opombe","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","(3) - Ta vrednost ne vključuje zmanjševanja zmogljivosti zaradi odmrzovanja.","(3) - Ta vrednost ne vključuje zmanjševanja zmogljivosti zaradi odmrzovanja."]
["Hladilna kapaciteta","Nom.","","kW","","24.1 (1)"]
["Grelna kapaciteta","Nom.","","kW","","26.4 (2)"]
["Hlajenje prostora","Zmogljivost","Pdizajn","kW","","24.1"]
["","SEER","","","","5.74"]
["","Letna poraba energije","","kWh/a","","2518"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","","12.1"]
["","SCOP/A","","","","3.76"]
["","Letna poraba energije","","kWh/a","","4484"]
["Razpon energetske učinkovitosti","","","","","A+++ ~ D"]