{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FBA71A2VEB / AZAS71M2V1B (Archived)"]
["Zunanja enota","","","","AZAS71M2V1B"]
["Hladilna kapaciteta","Nom.","","kW","6.80 (1)"]
["Grelna kapaciteta","Nom.","","kW","7.50 (2)"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A"]
["","Zmogljivost","Pdizajn","kW","6.80"]
["","SEER","","","5.57"]
["","Letna poraba energije","","kWh/a","427"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A"]
["","Zmogljivost","Pdizajn","kW","4.50"]
["","SCOP/A","","","3.81"]
["","Letna poraba energije","","kWh/a","1654"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D"]
["Opombe","","","","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]