{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":18,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FBA60A2VEB / FBA60A2VEB / RZQG125L8Y1B","FBA35A2VEB / FBA35A2VEB / RZQG71L8Y1B","FBA71A2VEB / RZQG71L8Y1B","FBA50A2VEB / FBA50A2VEB / RZQG71L8Y1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQG71L8Y1B","FBA50A2VEB / FBA50A2VEB / RZQG100L8Y1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQG100L8Y1B","FBA71A2VEB / FBA71A2VEB / RZQG100L8Y1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQG100L8Y1B","FBA50A2VEB / FBA50A2VEB / FBA50A2VEB / RZQG100L8Y1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQG125L8Y1B","FBA50A2VEB / FBA50A2VEB / FBA50A2VEB / RZQG125L8Y1B","FBA71A2VEB / FBA71A2VEB / RZQG125L8Y1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZQG140L7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","","6.80 (1)","6.80 (1)","","","9.50 (1)","9.50 (1)","","","","12.0 (1)","12.0 (1)","","13.4 (1)"]
["Hlajenje prostora","SEER","","","","5.10","6.16","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","5.10","","10.0"]
["","ηs,c","","%","","","","","","","","","","","","","","398.2"]
["","Letna poraba energije","","kWh/a","","466","386","467","466","652","652","652","652","652","824","824","","802"]
["","Zmogljivost","Pdizajn","kW","","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","12.0","12.0","","13.4"]
["","Razred energijske učinkovitosti","","","","A","A++","A","A","A","A","A","A","A","A","A"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","","6.00","6.00","6.00","6.00","11.3","11.3","11.3","11.3","11.3","12.7","12.7","","12.2"]
["","SCOP/A","","","","3.80","4.31","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80","","3.96"]
["","Razred energijske učinkovitosti","","","","A","A+","A","A","A","A","A","A","A","A","A"]
["","Letna poraba energije","","kWh/a","","2,210","1,949","2,211","2,210","4,163","4,163","4,164","4,164","4,164","4,683","4,683","","4,307"]
["","ηs,h","","%","","","","","","","","","","","","","","155.2"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","","","944"]
["","EER","","","","3.39 (3)","3.60 (3)","","","3.96 (3)","3.55 (3)","","","","3.21 (3)","3.02 (3)","","4.61 (3)"]
["","COP","","","","3.61 (3)","4.01 (3)","","","3.31 (3)","4.00 (3)","","","","3.57 (3)","3.54 (3)"]
["","Direktiva o energijskih oznakah","Hlajenje","","","A","A","","","A","A","","","","A","B"]
["","","Ogrevanje","","","A","A","","","A","A","","","","B","B"]
["Grelna kapaciteta","Nom.","","kW","","7.50 (2)","7.50 (2)","","","10.8 (2)","10.8 (2)","","","","13.5 (2)","13.5 (2)","","15.5 (2)"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D","","","","","","","","","","","","A+++ ~ D"]
["Zunanja enota","","","","","","","","","","","","","","","","RZQG125L8Y1"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","","","","","","","","","","","","A"]
["","Zmogljivost","Pdizajn","kW","","","","","","","","","","","","","12.0"]
["","SEER","","","","","","","","","","","","","","","5.10"]
["","Letna poraba energije","","kWh/a","","","","","","","","","","","","","824"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","","","","","","","","","","","","A"]
["","Zmogljivost","Pdizajn","kW","","","","","","","","","","","","","12.7"]
["","SCOP/A","","","","","","","","","","","","","","","3.80"]
["","Letna poraba energije","","kWh/a","","","","","","","","","","","","","4683"]