{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","37.0","37.0","31.0","31.0"]
["","","","Srednja","dBA","34.0","34.0","28.0","28.0"]
["","","","Nizko","dBA","29.0","29.0","25.0","25.0"]
["","Hlajenje","","Srednja","dBA","32.0","32.0","28.0","28.0"]
["","","","Nizko","dBA","29.0","29.0","25.0","25.0"]
["","","","Visok","dBA","35.0","35.0","30.0","30.0"]
["Standardni pripomočki","Priročnik za upravljanje","","","","1","1","1","1"]
["","Priročnik za namestitev","","","","1","1","1","1"]
["","Cev izpusta","","","","1","1","1","1"]
["","Kovinska objemka za izpustno cev","","","","1","1","1","1"]
["","Podložka za konzolo obešalnika","","","","8","8","8","8"]
["","Vijaki","","","","40","40","40","40"]
["","Izolacija za priključke","","","","2","2","2","2"]
["","Tesnilne plošče","","","","5","5","5","5"]
["","Objemke","","","","4","4","4","4"]
["Krmilni sistemi","Wired remote control","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Piping connections","Tekočina","","Zun. premer","mm","6.35","6.35","6.35","9.52"]
["","Plin","","Zun. premer","mm","9.52","12.70","12.70","15.90"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Raven zvočne moči","Hlajenje","","","dBA","60","60","56","56"]
["Mere","Enota","","Širina","mm","700","700","1,000","1,000"]
["","","","Globina","mm","800","800","800","800"]
["","","","Višina","mm","245","245","245","245"]
["Ohišje","Material","","","","Galvanizirana jeklena plošča","Galvanizirana jeklena plošča","Galvanizirana jeklena plošča","Galvanizirana jeklena plošča"]
["","Colour","","","","Brez barvanja (galvanizirano)","Brez barvanja (galvanizirano)","Brez barvanja (galvanizirano)","Brez barvanja (galvanizirano)"]
["Teža","Enota","","","kg","28.0","28.0","35.0","35.0"]
["Ventilator","Zunanji statični tlak","","Visok","Pa","150","150","150","150"]
["","","","Nom.","Pa","30","30","30","30"]
["","Hitrost pretoka zraka","Gretje","Visok","m³/min","15.0","15.0","18.0","18.0"]
["","","","Nizko","m³/min","10.5","10.5","12.5","12.5"]
["","","","Srednja","m³/min","12.5","12.5","15.0","15.0"]
["","","Hlajenje","Nizko","m³/min","10.5","10.5","12.5","12.5"]
["","","","Srednja","m³/min","12.5","12.5","15.0","15.0"]
["","","","Visok","m³/min","15.0","15.0","18.0","18.0"]
["Višina odvajanja","mm","","","","625","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","50/60","50/60","50/60","50/60"]
["","Napetost","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Opombe","","","","","(1) - Raven zvočne moči je absolutna vrednost, ki označuje moč, ki jo ustvarja vir zvoka.","(1) - Raven zvočne moči je absolutna vrednost, ki označuje moč, ki jo ustvarja vir zvoka.","(1) - Raven zvočne moči je absolutna vrednost, ki označuje moč, ki jo ustvarja vir zvoka.","(1) - Raven zvočne moči je absolutna vrednost, ki označuje moč, ki jo ustvarja vir zvoka."]
["","","","","","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke"]