{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-C8 / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FBQ71C8VEB / RZQG71L9V1B","FBQ100C8VEB / RZQG100L9V1B","FBQ35C8VEB / FBQ35C8VEB / RZQG71L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG100L9V1B","FBQ50C8VEB / FBQ50C8VEB / RZQG100L9V1B","FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / FBQ35C8VEB / RZQG125L9V1B","FBQ125C8VEB / RZQG125L9V1B","FBQ50C8VEB / FBQ50C8VEB / FBQ50C8VEB / RZQG125L9V1B","FBQ60C8VEB / FBQ60C8VEB / RZQG125L9V1B"]
["Hladilna kapaciteta","Nom.","","kW","6.8","9.5","","","","","12.0"]
["Hlajenje prostora","SEER","","","5.61, 6.11","5.80","5.10","5.10","5.10","5.10","5.81","5.10","5.10"]
["","Letna poraba energije","","kWh/a","390","574","467","652","652","824","723","824","824"]
["","Zmogljivost","Pdizajn","kW","6.80","9.50","6.80","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Razred energijske učinkovitosti","","","A++","A+","B","B","B","B","A+","B","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","6.00","11.30","6.00","11.30","11.30","12.71","12.71","12.71","12.71"]
["","SCOP/A","","","4.01","4.61","3.80","3.80","3.80","3.80","4.21","3.80","3.80"]
["","Razred energijske učinkovitosti","","","A+","A++","A","A","A","A","A+","A","A"]
["","Letna poraba energije","","kWh/a","2,095","3,432","2,211","4,164","4,164","4,683","4,227","4,683","4,683"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","970","1,220","","","","","1,575"]
["","EER","","","3.50","3.89","","","","","3.81"]
["","COP","","","3.65","4.21","","","","","3.83"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","","","","","A"]
["","","Ogrevanje","","A","A","","","","","A"]
["Grelna kapaciteta","Nom.","","kW","7.5","10.8","","","","","13.5"]
["Opombe","","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]