{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBQ35D2VEB / FBQ35D2VEB / RZQSG71L3V1B","FBQ71D2VEB / RZQSG71L3V1B (Preliminary)","FBQ50D2VEB / FBQ50D2VEB / RZQSG100L9V1B","FBQ100D2VEB / RZQSG100L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQSG100L9V1B","FBQ125D2VEB / RZQSG125L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQSG125L9V1B","FBQ60D2VEB / FBQ60D2VEB / RZQSG125L9V1B","FBQ140D2VEB / RZQSG140L9V1B"]
["Hlajenje prostora","SEER","","","5.10","5.84","5.10","5.61","5.10","5.47","4.80","4.80"]
["","Letna poraba energije","","kWh/a","467","408","652","593","652","768","875","875"]
["","Zmogljivost","Pdizajn","kW","6.80","6.80","9.50","9.50","9.50","12.00","12.00","12.00"]
["","Razred energijske učinkovitosti","","","A","A+","A","A+","A","A","B","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","6.00","6.00","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","4.10","3.80","4.15","3.80","4.01","3.80","3.80"]
["","Razred energijske učinkovitosti","","","A","A+","A","A+","A","A+","A","A"]
["","Letna poraba energije","","kWh/a","2,211","2,049","2,800","2,564","2,800","2,653","2,800","2,800"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]
["Hladilna kapaciteta","Nom.","","kW","","6.8","","9.5 (2)","","12.0 (2)","","","13.4 (2)"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","","1,030","","1,418","","1,858"]
["","EER","","","","3.30","","3.35 (1)","","3.23 (1)","","","3.06 (1)"]
["","COP","","","","3.81","","3.67 (1)","","3.63 (1)","","","3.40 (1)"]
["","Direktiva o energijskih oznakah","Hlajenje","","","A","","A","","A"]
["","","Ogrevanje","","","A","","A","","A"]
["Grelna kapaciteta","Nom.","","kW","","7.5","","10.80 (2)","","13.50 (2)","","","15.50 (2)"]
["Opombe","","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","","","","(3) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije","","(3) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije"]
["","","","","","","","(4) - SEER in SCOP sta v skladu z EN 14825","","(4) - SEER in SCOP sta v skladu z EN 14825"]