{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / AZAS100M7V1B","FCAG71AVEB / AZAS71M2V1B","FCAG125AVEB / AZAS125M7V1B","FCAG140AVEB / AZAS140M7V1B"]
["Hladilna kapaciteta","Nom.","","kW","","6.80 (1)","12.1 (1)","13.4 (1)"]
["Grelna kapaciteta","Nom.","","kW","","7.50 (2)","13.5 (2)","15.5 (2)"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","A+"]
["","Zmogljivost","Pdizajn","kW","","6.80","12.1","13.0"]
["","SEER","","","","5.87","5.40","6.00"]
["","Letna poraba energije","","kWh/a","","405","1,345","1,300"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","A"]
["","Zmogljivost","Pdizajn","kW","","4.50","6.00","7.80"]
["","SCOP/A","","","","4.00","3.80","4.31"]
["","Letna poraba energije","","kWh/a","","1,575","2,211","2,534"]
["Opombe","","","","","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m"]
["","","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["Razpon energetske učinkovitosti","","","","A+++ ~ D"]