{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / AZAS-MY1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / AZAS100M7Y1B","FCAG125AVEB / AZAS125M7Y1B","FCAG140AVEB / AZAS140M7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","","12.1 (1)","13.4 (1)"]
["Grelna kapaciteta","Nom.","","kW","","13.5 (2)","15.5 (2)"]
["Hlajenje prostora","Zmogljivost","Pdizajn","kW","","12.1","13.0"]
["","SEER","","","","5.40","6.00"]
["","Letna poraba energije","","kWh/a","","1,345","1,300"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","","6.00","7.80"]
["","SCOP/A","","","","3.80","4.31"]
["","Letna poraba energije","","kWh/a","","2,211","2,534"]
["Opombe","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["Zunanja enota","","","","AZAS100M7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","9.50 (1)"]
["Grelna kapaciteta","Nom.","","kW","10.8 (2)"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A+"]
["","Zmogljivost","Pdizajn","kW","9.50"]
["","SEER","","","5.67"]
["","Letna poraba energije","","kWh/a","586"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A"]
["","Zmogljivost","Pdizajn","kW","6.00"]
["","SCOP/A","","","3.85"]
["","Letna poraba energije","","kWh/a","2182"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D"]