{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":13,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FCAG71AVEB / RZASG71M2V1B","FCAG35AVEB / FCAG35AVEB / RZASG71M2V1B","FCAG100AVEB / RZASG100M7V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZASG100M7V1B","FCAG50AVEB / FCAG50AVEB / RZASG100M7V1B","FCAG125AVEB / RZASG125M7V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZASG125M7V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZASG140M7V1B","FCAG140AVEB / RZASG140M7V1B"]
["Outdoor unit","","","","RZASG71M2V1B","RZASG71M2V1B","RZASG100M7V1B","RZASG100M7V1B","RZASG100M7V1B","RZASG125M7V1B","RZASG125M7V1B","RZASG140M7V1B","RZASG140M7V1B"]
["Hladilna kapaciteta","Nom.","","kW","6.80","6.80","9.5","9.50","9.50","12.1","12.1","13.4","13.4 (1)"]
["Grelna kapaciteta","Nom.","","kW","7.50","7.50","10.8","10.8","10.8","13.5","13.5","15.5","15.5 (2)"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A++","A++","A++","A++","A++"]
["","Zmogljivost","Pdizajn","kW","6.80","6.80","9.5","9.50","9.50","12.1","12.1","13.4","13.4"]
["","SEER","","","6.47","7.05","6.5","7.22","6.80","5.76","9.47","11.6","6.53"]
["","Letna poraba energije","","kWh/a","368","338","507","461","489","1261","767","694","1231"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A","A+","A+","A+","A"]
["","Zmogljivost","Pdizajn","kW","4.50","4.50","6.0","6.00","6.00","6.00","6.00","7.80","7.80"]
["","SCOP/A","","","4.00","4.31","4.2","4.07","3.90","4.05","4.65","5.49","4.31"]
["","Letna poraba energije","","kWh/a","1575","1462","2016","2064","2154","2074","1807","1989","2534"]
["Opombe","","","","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["Razpon energetske učinkovitosti","","","","","","","","","","","","A+++ ~ D"]