{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":21,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG100L8Y1B","FCAG125AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG100L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / RZQG71L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG71L8Y1B","FCAG71AVEB / RZQG71L8Y1B","FCAG100AVEB / RZQG71L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG100L8Y1B","FCAG140AVEB / RZQG100L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG125L8Y1B","FCAG140AVEB / RZQG140L7Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L7Y1B"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Hlajenje prostora","SEER","","","","","","","","","","5.10","5.10","6.72","","","","","","6.44","9.70"]
["","Letna poraba energije","","kWh/a","","","","","","","","467","467","355","","","","","","1,249","829"]
["","Zmogljivost","Pdizajn","kW","","","","","","","","6.80","6.80","6.80","","","","","","13.4","13.4"]
["","Razred energijske učinkovitosti","","","","","","","","","","A","A","A++"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","","","","","","","","6.00","6.00","6.33","","","","","","11.6","12.0"]
["","SCOP/A","","","","","","","","","","3.80","3.80","4.20","","","","","","4.27","3.96"]
["","Razred energijske učinkovitosti","","","","","","","","","","A","A","A+"]
["","Letna poraba energije","","kWh/a","","","","","","","","2,211","2,211","2,110","","","","","","3,795","4,235"]
["Opombe","","","","","","","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","","","","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","","","","","","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["Hladilna kapaciteta","Nom.","","kW","","","","","","","","","","6.80 (1)","","","","","","13.4 (1)","13.4 (1)"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","","","","","","","","","","1,005"]
["","EER","","","","","","","","","","","","3.39 (3)","","","","","","2.50 (3)","4.29 (3)"]
["","COP","","","","","","","","","","","","3.97 (3)","","","","","","3.61 (3)"]
["","Direktiva o energijskih oznakah","Hlajenje","","","","","","","","","","","A"]
["","","Ogrevanje","","","","","","","","","","","A"]
["Grelna kapaciteta","Nom.","","kW","","","","","","","","","","7.50 (2)","","","","","","15.5 (2)","15.5 (2)"]
["Zunanja enota","","","","","","","","","","","","","","","RZQG100L8Y1","","RZQG125L8Y1"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","","","","","","","","","","","A","","A"]
["","Zmogljivost","Pdizajn","kW","","","","","","","","","","","","9.50","","12.0"]
["","SEER","","","","","","","","","","","","","","5.10","","5.10"]
["","Letna poraba energije","","kWh/a","","","","","","","","","","","","652","","824"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","","","","","","","","","","","A","","A"]
["","Zmogljivost","Pdizajn","kW","","","","","","","","","","","","11.3","","12.7"]
["","SCOP/A","","","","","","","","","","","","","","3.80","","3.80"]
["","Letna poraba energije","","kWh/a","","","","","","","","","","","","4164","","4683"]
["Hlajenje prostora","ηs,c","","%","","","","","","","","","","","","","","","","254.6","385.1"]
["Ogrevanje prostora (Povprečno podnebje)","ηs,h","","%","","","","","","","","","","","","","","","","167.6","155.2"]