{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQSG100L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG100L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQSG100L8Y1B","FCAG125AVEB / RZQSG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG125L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQSG125L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQSG125L8Y1B","FCAG140AVEB / RZQSG140L7Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQSG140L7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","9.50 (1)","","","12.0 (1)","","","","13.4 (1)","13.4 (1)"]
["Hlajenje prostora","SEER","","","6.50","5.10","5.10","5.30","4.80","4.80","4.80"]
["","Letna poraba energije","","kWh/a","512","652","652","793","875","875","875"]
["","Zmogljivost","Pdizajn","kW","9.50","9.50","9.50","12.0","12.0","12.0","12.0"]
["","Razred energijske učinkovitosti","","","A++","A","A","A","B","B","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","7.60","7.60","7.60","8.03","7.60","7.60","7.60"]
["","SCOP/A","","","4.10","3.80","3.80","4.01","3.80","3.80","3.80"]
["","Razred energijske učinkovitosti","","","A+","A","A","A+","A","A","A"]
["","Letna poraba energije","","kWh/a","2,596","2,800","2,800","2,804","2,800","2,800","2,800"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","1,440","","","1,870"]
["","EER","","","3.30 (3)","","","3.21 (3)","","","","2.40 (3)","4.20 (3)"]
["","COP","","","3.54 (3)","","","3.41 (3)","","","","3.41 (3)"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","","","A"]
["","","Ogrevanje","","A","","","B"]
["Grelna kapaciteta","Nom.","","kW","10.8 (2)","","","13.5 (2)","","","","15.5 (2)","15.5 (2)"]
["Opombe","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]