{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXM-N9"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXM35N2V1B9","FCAG35BVEB / RXM35N5V1B9","FCAG50BVEB / RXM50N2V1B9","FCAG60BVEB / RXM60N2V1B9"]
["Hladilna kapaciteta","Nom.","","kW","3.50","3.50","5.00","5.70"]
["Grelna kapaciteta","Nom.","","kW","4.20","4.20","6.00","7.00"]
["Nazivna učinkovitost","EER","","","3.72","3.72","3.58","3.31"]
["","COP","","","3.77","3.77","3.70","3.38"]
["","Letna por.energ.","","kWh","470","470","698","861"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","A","A"]
["","","Ogrevanje","","A","A","A","C"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A++","A++","","A++"]
["","Zmogljivost","Pdizajn","kW","3.50","3.50","","5.70"]
["","SEER","","","6.35","6.35","","6.40"]
["","Letna poraba energije","","kWh/a","193","193","","312"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A++","A++","","A+"]
["","Zmogljivost","Pdizajn","kW","3.32","3.32","","4.71"]
["","SCOP/A","","","4.90","4.90","","4.20"]
["","Letna poraba energije","","kWh/a","948","948","","1,569"]
["Opombe","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke"]