{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RXS50L2V1B","FCAG60BVEB / RXS60L2V1B"]
["Hladilna kapaciteta","Nom.","","kW","5.00","5.70"]
["Grelna kapaciteta","Nom.","","kW","6.00","7.00"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","EER","","","3.55","3.48"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A"]
["","","Ogrevanje","","A","B"]
["Priključki cevne napeljave","Drain","OD","mm","VP25 (Zunanji premer 32, notranji premer 25)","VP25 (Zunanji premer 32, notranji premer 25)"]
["","Plin","Zun. premer","mm","12.70","12.70"]
["","Tekočina","Zun. premer","mm","6.35","6.35"]
["Opombe","","","","(1) - Pri normalnem obratovanju: +22 °C / +32 °C","(1) - Pri normalnem obratovanju: +22 °C / +32 °C"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke"]