{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":23,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["Grelna kapaciteta","Nom.","","kW","","","","","","","","","","","","","","","","","","7.50","15.50"]
["Nazivna učinkovitost","EER","","","","","","","","","","","","","","","","3.30","3.30","3.30","3.39","3.39","2.50"]
["","COP","","","","","","","","","","","","","","","","","","","","3.97","3.61"]
["","Letna por.energ.","","kWh","","","","","","","","","","","","","","","","","","1,003"]
["","Direktiva o energijskih oznakah","Hlajenje","","","","","","","","","","","","","","","","","","","A"]
["","","Ogrevanje","","","","","","","","","","","","","","","","","","","A"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","","","","","","","","","","","","","A","A","A","A++","A++"]
["","Zmogljivost","Pdizajn","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["","SEER","","","","","","","","","","","","","","","","5.10","5.10","5.10","6.80","6.72","6.44"]
["","Letna poraba energije","","kWh/a","","","","","","","","","","","","","","467","467","467","350","355","1,249"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","","","","","","","","","","","","","A","A","A","A+","A+"]
["","Zmogljivost","Pdizajn","kW","","","","","","","","","","","","","","6.00","6.00","6.00","6.33","6.33","11.56"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","3.80","3.80","4.20","4.20","4.27"]
["","Letna poraba energije","","kWh/a","","","","","","","","","","","","","","2,211","2,211","2,211","2,110","2,110","3,795"]
["Opombe","","","","","","","","","","","","","","","","","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Glejte ločeno risbo za obratovalno območje","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","","","","","","","","","","","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke","(2) - Glejte ločeno risbo za električne podatke","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","","","","","","","","","","","","","","(3) - Glejte ločeno risbo za obratovalno območje","","","","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","","","","","","","","","","","","","(4) - Glejte ločeno risbo za električne podatke","","","","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]