{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":12,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZQG100L8Y1B","FCAHG125GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG100L8Y1B","FCAHG140GVEB / RZQG125L8Y1B","FCAHG71GVEB / RZQG71L8Y1B","FCAHG100GVEB / RZQG71L8Y1B","FCAHG71GVEB / FCAHG71GVEB / RZQG125L8Y1B","FCAHG140GVEB / RZQG140L7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","","","","","6.80 (1)","","","13.4 (1)"]
["Hlajenje prostora","SEER","","","","","","","6.91","6.91","","6.75"]
["","ηs,c","","%","","","","","","","","266.9"]
["","Letna poraba energije","","kWh/a","","","","","345","345","","1,191"]
["","Zmogljivost","Pdizajn","kW","","","","","6.80","6.80","","13.4"]
["","Razred energijske učinkovitosti","","","","","","","A++","A++"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","","","","","7.60","7.60","","11.8"]
["","SCOP/A","","","","","","","4.54","4.54","","4.38"]
["","Razred energijske učinkovitosti","","","","","","","A+","A+"]
["","Letna poraba energije","","kWh/a","","","","","2,344","2,344","","3,766"]
["","ηs,h","","%","","","","","","","","172.1"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","","","","","830"]
["","EER","","","","","","","4.09 (3)","","","3.18 (3)"]
["","COP","","","","","","","4.80 (3)","","","4.12 (3)"]
["","Direktiva o energijskih oznakah","Hlajenje","","","","","","A"]
["","","Ogrevanje","","","","","","A"]
["Grelna kapaciteta","Nom.","","kW","","","","","7.50 (2)","","","15.5 (2)"]
["Opombe","","","","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","","","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","A+++ ~ D"]
["Zunanja enota","","","","","","","","","","RZQG125L8Y1"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","","","","","","A"]
["","Zmogljivost","Pdizajn","kW","","","","","","","12.0"]
["","SEER","","","","","","","","","5.10"]
["","Letna poraba energije","","kWh/a","","","","","","","824"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","","","","","","A"]
["","Zmogljivost","Pdizajn","kW","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","3.80"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","","","","","","","11.4"]
["","Letna poraba energije","","kWh/a","","","","","","","4683"]