{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":8,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FCAHG71GVEB / RZQSG71L3V1B","FCAHG100GVEB / RZQSG100L9V1B","FCAHG125GVEB / RZQSG125L9V1B","FCAHG140GVEB / RZQSG140L9V1B"]
["Hladilna kapaciteta","Nom.","","kW","6.80 (1)","9.50 (1)","12.0 (1)","13.4 (1)"]
["Hlajenje prostora","SEER","","","6.50","6.70","5.40"]
["","Letna poraba energije","","kWh/a","367","497","778"]
["","Zmogljivost","Pdizajn","kW","6.80","9.50","12.0"]
["","Razred energijske učinkovitosti","","","A++","A++","A"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","7.60","8.03","8.03"]
["","SCOP/A","","","4.15","4.30","4.10"]
["","Razred energijske učinkovitosti","","","A+","A+","A+"]
["","Letna poraba energije","","kWh/a","2,563","2,615","2,742"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","970","1,285","1,855"]
["","EER","","","3.50 (3)","3.70 (3)","3.23 (3)","3.11 (3)"]
["","COP","","","4.10 (3)","4.30 (3)","3.75 (3)","3.61 (3)"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","A"]
["","","Ogrevanje","","A","A","A"]
["Grelna kapaciteta","Nom.","","kW","7.50 (2)","10.8 (2)","13.5 (2)","15.5 (2)"]
["Opombe","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]