{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RXS-J"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / RXS35J2V1B","FCQG50FVEB / RXS50J2V1B"]
["Hladilna kapaciteta","Nom.","","kW","3.40 (3)","5.00 (3)"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","475","705"]
["","EER","","","3.58","3.55"]
["","COP","","","3.41","3.70"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A"]
["","","Ogrevanje","","B","A"]
["Grelna kapaciteta","Nom.","","kW","4.20 (4)","6.00 (4)"]
["Opombe","","","","(1) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)","(1) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)"]
["","","","","(2) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)","(2) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)"]
["","","","","(3) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(3) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m"]
["","","","","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m"]
["","","","","(5) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(5) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]