{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":12,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQG50FVEB / FCQG50FVEB / RZQSG100L8Y1B","FCQG100FVEB / RZQSG100L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L8Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L8Y1B","FCQG125FVEB / RZQSG125L8Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L8Y1B","FCQG60FVEB / FCQG60FVEB / RZQSG125L8Y1B","FCQG140FVEB / RZQSG140L7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","","9.5","","","12.0","","","13.4"]
["Hlajenje prostora","SEER","","","5.1","6.5","5.1","4.8","5.3","4.8","4.8"]
["","Letna poraba energije","","kWh/a","652","512","652","875","793","875","875"]
["","Zmogljivost","Pdizajn","kW","9.5","9.5","9.5","12","12","12","12"]
["","Razred energijske učinkovitosti","","","B","A++","B","B","A","B","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","7.6","7.6","7.6","7.6","8.03","7.6","7.6"]
["","SCOP/A","","","3.8","4.1","3.8","3.8","4.01","3.8","3.8"]
["","Razred energijske učinkovitosti","","","A","A+","A","A","A+","A","A"]
["","Letna poraba energije","","kWh/a","2,800","2,596","2,800","2,800","2,804","2,800","2,800"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","","1,440","","","1,870","","","2,225"]
["","EER","","","","3.30","","","3.21","","","3.01"]
["","COP","","","","3.54","","","3.41","","","3.41"]
["","Direktiva o energijskih oznakah","Hlajenje","","","A","","","A"]
["","","Ogrevanje","","","A","","","B"]
["Grelna kapaciteta","Nom.","","kW","","10.8","","","13.5","","","15.5"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]
["","","","","","(3) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije","","","(3) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije"]
["","","","","","(4) - SEER in SCOP sta v skladu z EN 14825","","","(4) - SEER in SCOP sta v skladu z EN 14825"]