{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":22,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FCQG35FVEB / FCQG35FVEB / RZQSG71L2V1B","FCQG71FVEB / RZQSG71L2V1B","FCQG100FVEB / RZQSG100L7V1B","FCQG100FVEB / RZQSG100L7Y1B","FCQG100FVEB / RZQSG100L7Y1B9","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L7V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG100L7Y1B9","FCQG50FVEB / FCQG50FVEB / RZQSG100L7V1B","FCQG50FVEB / FCQG50FVEB / RZQSG100L7Y1B9","FCQG125FVEB / RZQSG125L7Y1B9","FCQG125FVEB / RZQSG125L7V1B","FCQG125FVEB / RZQSG125L7Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L7V1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQSG125L7Y1B9","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L7V1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQSG125L7Y1B9","FCQG60FVEB / FCQG60FVEB / RZQSG125L7V1B","FCQG60FVEB / FCQG60FVEB / RZQSG125L7Y1B9"]
["Hladilna kapaciteta","Nom.","","kW","","6.8","9.5","9.5 (3)","9.5","","","","","12.0","12.0","12.0 (3)"]
["Hlajenje prostora","SEER","","","4.30","5.11","5.11","5.11 (6)","5.11","4.30","4.30","4.30","4.30","5.11","5.11","5.11 (6)","4.00","4.00","4.30","4.30","4.30","4.30"]
["","Letna poraba energije","","kWh/a","554","466","650.685","","650.685","773.256","773.256","773.256","773.256","821.918","821.918","","1,050","1,050","976.744","976.744","976.744","976.744"]
["","Zmogljivost","Pdizajn","kW","6.80","6.80","9.50","","9.50","9.50","9.50","9.50","9.50","12.00","12.00","","12.00","12.00","12.00","12.00","12.00","12.00"]
["","Razred energijske učinkovitosti","","","C","A","A","","A","C","C","C","C","A","A","","D","D","C","C","C","C"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","6.00","6.33","7.60","","7.60","6.81","6.81","6.81","6.81","8.03","8.03","","8.03","8.03","8.03","8.03","8.03","8.03"]
["","SCOP/A","","","3.40","3.81","3.80","3.80 (6)","3.80","3.40","3.40","3.40","3.40","3.81","3.81","3.81 (6)","3.40","3.40","3.40","3.40","3.40","3.40"]
["","Razred energijske učinkovitosti","","","A","A","A","","A","A","A","A","A","A","A","","A","A","A","A","A","A"]
["","Letna poraba energije","","kWh/a","2,472","2,327","2,799","","2,799","2,802","2,802","2,802","2,802","2,949","2,949","","3,305","3,305","3,305","3,305","3,306.471","3,306.471"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","","971","1,440","1,440","1,440","","","","","1,870","1,870","1,870"]
["","EER","","","","3.21","3.30","3.30","3.30","","","","","3.21","3.21","3.21"]
["","COP","","","","3.61","3.54","3.54","3.54","","","","","3.41","3.41","3.41"]
["","Direktiva o energijskih oznakah","Hlajenje","","","A","A","A","A","","","","","A","A","A"]
["","","Ogrevanje","","","A","B","A","B","","","","","B","B","B"]
["Grelna kapaciteta","Nom.","","kW","","7.5","10.8","10.8 (4)","10.8","","","","","13.5","13.5","13.5 (4)"]
["Opombe","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)"]
["","","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)"]
["","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","","","","(3) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","","","","","","","","(3) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m"]
["","","","","","","","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m","","","","","","","","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m"]
["","","","","","","","(5) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije","","","","","","","","(5) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije"]
["","","","","","","","(6) - SEER in SCOP sta v skladu z EN 14825","","","","","","","","(6) - SEER in SCOP sta v skladu z EN 14825"]
["","","","","","","","(7) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","","","","","","(7) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]