{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQSG-L(3/8)V1"]
[]
[]
[]
[]
["","","","","FCQHG100FVEB / RZQSG100L8V1B","FCQHG125FVEB / RZQSG125L8V1B","FCQHG140FVEB / RZQSG140L7V1B"]
["Hladilna kapaciteta","Nom.","","kW","9.5","12.0","13.4"]
["Hlajenje prostora","SEER","","","6.70","5.40"]
["","Letna poraba energije","","kWh/a","496.269","777.778"]
["","Zmogljivost","Pdizajn","kW","9.50","12.00"]
["","Razred energijske učinkovitosti","","","A++","A"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","8.03","8.03"]
["","SCOP/A","","","4.30","4.10"]
["","Razred energijske učinkovitosti","","","A+","A+"]
["","Letna poraba energije","","kWh/a","2,614.419","2,741"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","1,285","1,855","2,085"]
["","EER","","","3.70","3.23","3.21"]
["","COP","","","4.30","3.75","3.61"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A"]
["","","Ogrevanje","","A","A"]
["Grelna kapaciteta","Nom.","","kW","10.8","13.5","15.5"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]