{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Hladilna kapaciteta","Skupna kapaciteta","","Nom.","kW","12.10","19.00","22.00"]
["Grelna kapaciteta","Total capacity","","Nom.","kW","13.50","22.4","24.0"]
["Casing","Barva","","","","Neprebarvano","Neprebarvano","Neprebarvano"]
["","Material","","","","Galvanizirano jeklo","Galvanizirana jeklena plošča","Galvanizirana jeklena plošča"]
["Mere","Enota","","Višina","mm","300","470","470"]
["","","","Širina","mm","1,400","1,490","1,490"]
["","","","Globina","mm","700","1,100","1,100"]
["Teža","Enota","","","kg","45","104","115"]
["Zahtevan prostor v stropu >","mm","","","","350"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50","56"]
["","","","Nizko","m³/min","28.0","36.0","43.0"]
["","","Ogrevanje","Visok","m³/min","39.0","64.0","69.0"]
["","","","Medium","m³/min","","50.0","56.0"]
["","","","Nizko","m³/min","28.0","36.0","43.0"]
["","Zunanji statični tlak","","Visok","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Raven zvočne moči","Hlajenje","","","dBA","66","69.0","71.0"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","40","43.0","44.0"]
["","","","Medium","dBA","","39.0","40.0"]
["","","","Nizko","dBA","33","36.0","37.0"]
["","Gretje","","Visok","dBA","40","43.0","44.0"]
["","","","Srednja","dBA","","39.0","40.0"]
["","","","Nizko","dBA","33","36.0","37.0"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","9.52","9.52","9.52"]
["","Plin","","Zun. premer","mm","15.90","19.1","22.2"]
["","priključka","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Višina odvajanja","mm","","","","625"]
["Dekorativna plošča","Model","","","","BYBS125DJW1"]
["","Barva","","","","Bela (10Y9/0,5)"]
["","Mere","","Višina","mm","55"]
["","","","Širina","mm","1,500"]
["","","","Globina","mm","500"]
["","Teža","","","kg","6.5"]
["Control systems","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardni pripomočki","Vijaki","","","","16","2","2"]
["","Podložka","","","","8","12","12"]
["","Cevna objemka","","","","1"]
["","Cev izpusta","","","","1"]
["","Splošni varnostni previdnostni ukrepi","","","","1","1","1"]
["","Priročnik za namestitev in upravljanje","","","","1","1","1"]
["","Žica za skupno električno napajanje","","","","2"]
["","Tesnilni material (izpustna cev)","","","","1"]
["","Tesnilni material","","","","2"]
["","Termalna izolacijska cev (tekočina)","","","","1"]
["","Termalna izolacijska cev (plin)","","","","1"]
["Power supply","Ime","","","","","VE","VE"]
["","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50/60","50/60","50/60"]
["","Napetost","","","V","220-240/220","220-240/220","220-240/220"]
["Opombe","","","","","(1) - Glejte ločeno risbo za električne podatke"]
["Standardni pripomočki","Priročnik za upravljanje","","","","","1","1"]
["","Priročnik za namestitev","","","","","1","1"]
["","Cev za plinski priključek","","","","","1","1"]
["","Material žične objemke","","","","","1","1"]
["","Vzmetna podložka","","","","","2","2"]
["","Vijak+Podložka","","","","","45","45"]
["","Vijak s šesterokotno glavo s podložko","","","","","49","49"]
["","Vijak s šesterokotno glavo","","","","","2","2"]
["","Navadna podložka","","","","","8","8"]