{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","35.0","35.0"]
["","","","Nizko","dBA","29.0","29.0"]
["","Hlajenje","","Nizko","dBA","28.0","28.0"]
["","","","Visok","dBA","35.0","35.0"]
["Standardni pripomočki","Priročnik za namestitev in upravljanje","","","","1","1"]
["","Sesalni zračni filter","","","","1","1"]
["Krmilni sistemi","Ožičeni daljinski krmilnik","","","","BRC1D52, BRC1E52A/B"]
["Priključki napeljave","Tekočina","","Zun. premer","mm","6.35"]
["","Plin","","Zun. premer","mm","9.52"]
["","priključka","","","","27.2"]
["Raven zvočne moči","Hlajenje","","","dBA","55","55"]
["","Gretje","","","dBA","55","55"]
["Mere","Enota","","Širina","mm","652","652"]
["","","","Globina","mm","502","502"]
["","","","Višina","mm","230","230"]
["Ohišje","Material","","","","S cinkom premazano nizkokarbonsko jeklo","S cinkom premazano nizkokarbonsko jeklo"]
["Teža","Enota","","","kg","17.0","17.0"]
["Ventilator","Hitrost pretoka zraka","Ogrevanje","Visok","m³/min","","6.95"]
["","","","Nizko","m³/min","","5.20"]
["","","Hlajenje","Nizko","m³/min","","5.20"]
["","","","Visok","m³/min","","6.50"]
["Power supply","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Ime","","","","V1","V1"]
["","Napetost","","","V","230","230 +/-10%"]
["Opombe","","","","","(1) - Zvočne vrednosti se merijo v prostoru izoliranem od odmeva.","(1) - Zvočne vrednosti se merijo v prostoru izoliranem od odmeva."]
["","","","","","(2) - Nivo tlaka zvoka je relativna vrednost, odvisna od oddaljenosti in akustike okolja. Za več informacij, prosimo poglejte skice o nivojih zvoka.","(2) - Nivo tlaka zvoka je relativna vrednost, odvisna od oddaljenosti in akustike okolja. Za več informacij, prosimo poglejte skice o nivojih zvoka."]
["","","","","","(3) - Raven zvočne moči je absolutna vrednost, ki označuje moč, ki jo ustvarja vir zvoka.","(3) - Raven zvočne moči je absolutna vrednost, ki označuje moč, ki jo ustvarja vir zvoka."]
["Priključki napeljave","Tekočina","","Zun. premer","mm","","6.35"]
["","Plin","","Zun. premer","mm","","9.52"]
["","priključka","","","","","27.2"]