{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":5,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RQ-BW1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RQ125B8W1B"]
["Hladilna kapaciteta","Nom.","","kW","12.5 (6)"]
["Priključki cevne napeljave","Tekočina","Zun. premer","mm","9.52"]
["","Plin","Zun. premer","mm","15.9"]
["","priključka","OD","mm","26"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","2,395"]
["","EER","","","2.61"]
["","COP","","","3.24"]
["","Direktiva o energijskih oznakah","Hlajenje","","D"]
["","","Ogrevanje","","C"]
["Grelna kapaciteta","Nom.","","kW","14.6 (7)"]
["Opombe","","","","(1) - Nivo tlaka zvoka je relativna vrednost, odvisna od oddaljenosti in akustike okolja. Za več informacij, prosimo poglejte skice o nivojih zvoka."]
["","","","","(2) - Raven zvočne moči je absolutna vrednost, ki označuje moč, ki jo ustvarja vir zvoka."]
["","","","","(3) - Zvočne vrednosti se merijo v prostoru izoliranem od odmeva."]
["","","","","(4) - Grelna kapaciteta velja samo za kombinacijo z zunanjo enot s toplotno črpalko"]
["","","","","(5) - V primeru odtočne napeljave za zunanjo enoto je potreben komplet za odtočno napeljavo (opcija)."]
["","","","","(6) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","(7) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","(8) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]