{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RQ-BW1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RQ125B8W1B","FDQ125C7VEB / RQ125B8W1B"]
["Hladilna kapaciteta","Nom.","","kW","12.2 (3)","12.2 (3)"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","2,260","2,260"]
["","EER","","","2.70","2.70"]
["","COP","","","3.30","3.30"]
["","Direktiva o energijskih oznakah","Hlajenje","","D","D"]
["","","Ogrevanje","","C","C"]
["Grelna kapaciteta","Nom.","","kW","14.5 (4)","14.5 (4)"]
["Opombe","","","","(1) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)","(1) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)"]
["","","","","(2) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)","(2) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)"]
["","","","","(3) - Hlajenje: notranja temp. 27 °CDB, 19,0 °CWB; zunanja temp. 35°CDB; ekvivalentna dolžina cevi: 7,5 m; višinska razlika: 0 m","(3) - Hlajenje: notranja temp. 27 °CDB, 19,0 °CWB; zunanja temp. 35°CDB; ekvivalentna dolžina cevi: 7,5 m; višinska razlika: 0 m"]
["","","","","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","(5) - Skladno z EN/IEC 61000-3-11 oziroma EN/IEC 61000-3-12 se je mogoče treba obrniti na distributerja elektrike, da se zagotovi, da je oprema priklopljena samo na napajanje z Zsys (sistemska impedanca) ≤ Zmax oziroma da je Ssc≥ od minimalne vrednosti Ssc.","(5) - Skladno z EN/IEC 61000-3-11 oziroma EN/IEC 61000-3-12 se je mogoče treba obrniti na distributerja elektrike, da se zagotovi, da je oprema priklopljena samo na napajanje z Zsys (sistemska impedanca) ≤ Zmax oziroma da je Ssc≥ od minimalne vrednosti Ssc."]
["","","","","(6) - Evropski/mednarodni tehnični standard, ki postavlja omejitve za spremembe napetosti, nihanja napetosti in migetanje v javnih nizkonapetostnih napajalnih sistemih za opremo, ki je deklarirana za tok ≤ 75A","(6) - Evropski/mednarodni tehnični standard, ki postavlja omejitve za spremembe napetosti, nihanja napetosti in migetanje v javnih nizkonapetostnih napajalnih sistemih za opremo, ki je deklarirana za tok ≤ 75A"]
["","","","","(7) - sistemska impedanca","(7) - sistemska impedanca"]
["","","","","(8) - Oprema je skladna z EN 61000-3-12: Evropski/mednarodni tehnični standard, ki postavlja omejitve za harmonske tokove, ki jih proizvaja oprema, priklopljena na javni nizkonapetostni sistem z vhodnimi tokovi >16A in ≤ 75A na fazo","(8) - Oprema je skladna z EN 61000-3-12: Evropski/mednarodni tehnični standard, ki postavlja omejitve za harmonske tokove, ki jih proizvaja oprema, priklopljena na javni nizkonapetostni sistem z vhodnimi tokovi >16A in ≤ 75A na fazo"]
["","","","","(9) - Kratkostična moč","(9) - Kratkostična moč"]
["","","","","(10) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(10) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]