{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDQ125C5VEB / RZQSG125L8Y1B","FDQ125C7VEB / RZQSG125L8Y1B"]
["Zmogljivost hlajenja","Nom.","","kW","12.0","12.0"]
["Hlajenje prostora","SEER","","","5.2","5.2"]
["","Letna poraba energije","","kWh/a","808","808"]
["","Zmogljivost","Pdizajn","kW","12","12"]
["","Razred energijske učinkovitosti","","","A","A"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","7.6","7.6"]
["","SCOP/A","","","3.9","3.9"]
["","Razred energijske učinkovitosti","","","A","A"]
["","Letna poraba energije","","kWh/a","2,729","2,729"]
["Nazivna učinkovitost","Annual energy consumption","","kWh","1,870","1,870"]
["","EER","","","3.21","3.21"]
["","COP","","","3.51","3.51"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A"]
["","","Ogrevanje","","B","B"]
["Grelna kapaciteta","Nom.","","kW","13.5","13.5"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]