{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":8,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-M9"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B / RXM25M3V1B9","FDXM35F3V1B / RXM35M3V1B9","FDXM50F3V1B / RXM50M3V1B9","FDXM60F3V1B / RXM60M3V1B9"]
["Hladilna kapaciteta","Min.","","kW","","1.40","","1.70"]
["","Maks.","","kW","","3.80","","6.50"]
["","Nom.","","kW","","3.40","","6.00"]
["Hlajenje prostora","SEER","","","","5.26","","5.56"]
["","Letna poraba energije","","kWh/a","","226","","315"]
["","Zmogljivost","Pdizajn","kW","","3.40","","6.00"]
["","Razred energijske učinkovitosti","","","","A","","A"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","","2.90","","4.60"]
["","SCOP/A","","","","3.88","","3.80"]
["","Razred energijske učinkovitosti","","","","A","","A"]
["","Letna poraba energije","","kWh/a","","1,046","","1,693"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","","570","","1,024"]
["","EER","","","","2.98","","2.93"]
["","COP","","","","3.48","","3.21"]
["","Direktiva o energijskih oznakah","Hlajenje","","","C","","C"]
["","","Ogrevanje","","","B","","C"]
["Grelna kapaciteta","Nom.","","kW","","4.00","","7.00"]
["","Min.","","kW","","1.40","","1.70"]
["","Maks.","","kW","","5.00","","7.10"]
["Opombe","","","","(1) - Glejte ločeno risbo za električne podatke","(1) - Glejte ločeno risbo za električne podatke","","(1) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(2) - Glejte ločeno risbo za obratovalno območje","(2) - Glejte ločeno risbo za obratovalno območje","","(2) - Glejte ločeno risbo za električne podatke"]
["","","","","(3) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(3) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","","(3) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(4) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(4) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","","(4) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["Outdoor unit","","","","RXM25M3V1B9","","RXM50M3V1B9"]
["Hladilna kapaciteta","Min.","","kW","1.30","","1.70"]
["","Nom.","","kW","2.40","","5.00"]
["","Maks.","","kW","3.00","","5.30"]
["Grelna kapaciteta","Min.","","kW","1.30","","1.70"]
["","Nom.","","kW","3.20","","5.80"]
["","Maks.","","kW","4.50","","6.00"]
["Nom. učink.","EER","","","3.77","","3.06"]
["","COP","","","4.00","","3.10"]
["","Letna por.energ.","","kWh","318","","816"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","A","","B"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","A","","D"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A+","","A+"]
["","Zmogljivost","Pdizajn","kW","2.40","","5.00"]
["","SEER","","","5.68","","5.77"]
["","Letna poraba energije","","kWh/a","148","","303"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A+","","A"]
["","Zmogljivost","Pdizajn","kW","2.60","","4.00"]
["","SCOP/A","","","4.24","","3.93"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","2.16","","3.55"]
["","Letna poraba energije","","kWh/a","858","","1424"]