{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RZAG-MY1"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / FDXM50F3V1B / RZAG71M7Y1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG71M7Y1B","FDXM35F3V1B / FDXM35F3V1B / RZAG71M7Y1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG100M7Y1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG100M7Y1B","FDXM50F3V1B / FDXM50F3V1B / FDXM50F3V1B / RZAG100M7Y1B","FDXM50F3V1B / FDXM50F3V1B / RZAG100M7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","6.80 (1)","6.80 (1)","6.80 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)"]
["Hlajenje prostora","Letna poraba energije","","kWh/a","334","377","380","423","416","379","387"]
["","Zmogljivost","Pdizajn","kW","6.80","6.80","6.80","9.50","9.50","9.50","9.50"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","4.70","4.70","4.70","7.80","7.80","7.80","7.80"]
["","Letna poraba energije","","kWh/a","1,485","1,537","1,589","2,540","2,438","2,324","2,421"]
["Grelna kapaciteta","Nom.","","kW","7.50 (2)","7.50 (2)","7.50 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)"]
["Hlajenje prostora","SEER","","","7.12","6.32","6.27","7.86","8.00","8.77","8.60"]
["","Razred energijske učinkovitosti","","","A++","A++","A++","A++","A++","A+++","A+++"]
["Ogrevanje prostora (Povprečno podnebje)","SCOP/A","","","4.43","4.28","4.14","4.30","4.48","4.70","4.51"]
["","Razred energijske učinkovitosti","","","A+","A+","A+","A+","A+","A++","A+"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]