{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B / FDXM35F3V1B / RZASG71M2V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZASG100M7V1B","FDXM50F3V1B / FDXM50F3V1B / RZASG100M7V1B"]
["Outdoor unit","","","","RZASG71M2V1B","RZASG100M7V1B","RZASG100M7V1B"]
["Hladilna kapaciteta","Nom.","","kW","6.80","9.50","9.50"]
["Grelna kapaciteta","Nom.","","kW","7.50","10.8","10.8"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A++","A++","A++"]
["","Zmogljivost","Pdizajn","kW","6.80","9.50","9.50"]
["","SEER","","","6.30","6.43","7.68"]
["","Letna poraba energije","","kWh/a","378","517","433"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A+","A","A"]
["","Zmogljivost","Pdizajn","kW","4.50","6.00","6.00"]
["","SCOP/A","","","4.22","3.89","3.93"]
["","Letna poraba energije","","kWh/a","1493","2159","2137"]
["Opombe","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]