{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":14,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B / FDXM35F3V1B / RZQG71L9V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZQG71L9V1B","FDXM50F3V1B / FDXM50F3V1B / RZQG71L9V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZQG100L9V1B","FDXM50F3V1B / FDXM50F3V1B / RZQG100L9V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZQG100L9V1B","FDXM50F3V1B / FDXM50F3V1B / FDXM50F3V1B / RZQG100L9V1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZQG125L9V1B","FDXM50F3V1B / FDXM50F3V1B / FDXM50F3V1B / RZQG125L9V1B","FDXM60F3V1B / FDXM60F3V1B / RZQG125L9V1B"]
["Hlajenje prostora","SEER","","","4.80","4.80","4.80","5.10","5.10","5.10","5.10","5.10","5.10","5.10"]
["","Letna poraba energije","","kWh/a","496","496","496","652","652","652","652","824","824","824"]
["","Zmogljivost","Pdizajn","kW","6.80","6.80","6.80","9.50","9.50","9.50","9.50","12.0","12.0","12.0"]
["","Razred energijske učinkovitosti","","","B","B","B","A","A","A","A","A","A","A"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","6.00","6.00","6.00","10.7","11.3","10.74","11.30","11.3","12.7","12.7"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Razred energijske učinkovitosti","","","A","A","A","A","A","A","A","A","A","A"]
["","Letna poraba energije","","kWh/a","2,211","2,211","2,211","3,957","4,164","3,957","4,164","4,164","4,683","4,683"]
["Opombe","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 7,5m, nivojska razlika: 0m"]
["","","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(3) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]