{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / 3MXM-N"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / FDXM25F3V1B9 / 3MXM52N2V1B"]
["Hladilna kapaciteta","Nom.","","kW","5.0"]
["Hlajenje prostora","SEER","","","6.36"]
["","Letna poraba energije","","kWh/a","276"]
["","Zmogljivost","Pdizajn","kW","5.00"]
["","Razred energijske učinkovitosti","","","A++"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","4.80"]
["","SCOP/A","","","3.83"]
["","Razred energijske učinkovitosti","","","A"]
["","Letna poraba energije","","kWh/a","1,754"]
["Nazivna učinkovitost","Annual energy consumption","","kWh","606"]
["","EER","","","4.12"]
["","COP","","","3.69"]
["","Direktiva o energijskih oznakah","Hlajenje","","A"]
["","","Ogrevanje","","A"]
["Grelna kapaciteta","Nom.","","kW","6.80"]
["Opombe","","","","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(4) - Glejte ločeno risbo za električne podatke"]