{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","35.0","35.0","","38.0"]
["","","","Srednja","dBA","33.0","33.0","","35.0"]
["","","","Nizko","dBA","27.0","27.0","","30.0"]
["","Hlajenje","","Medium","dBA","33.0","33.0","","35.0"]
["","","","Nizko","dBA","27.0","27.0","","30.0"]
["","","","Visok","dBA","35.0","35.0","","38.0"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","1","","1"]
["","Priročnik za upravljanje","","","","1","1","","1"]
["","Izolacija za priključke","","","","1","1","","1"]
["","Tesnilna plošča","","","","1","1","","1"]
["","Objemka, kovinska","","","","1","1","","1"]
["","Cev izpusta","","","","1","1","","1"]
["","Podložka za konzolo obešalnika","","","","8","8","","8"]
["","Tesnilni material","","","","2","2","","2"]
["","Objemke","","","","6","6","","6"]
["","Pritrdilna plošča podložke","","","","4","4","","4"]
["","Vijaki za prirobnice kanala","","","","1","1","","1"]
["","Zračni filter","","","","1","1","","1"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35","","6.35"]
["","Plin","","Zun. premer","mm","9.50","9.50","","12.70"]
["","priključka","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.036","0.036","","0.060"]
["","Gretje","","Nom.","kW","0.036","0.036","","0.060"]
["Raven zvočne moči","Hlajenje","","","dBA","53.0","53.0","","56.0"]
["","Gretje","","","dBA","53.0","53.0","","56.0"]
["Mere","Enota","","Width","mm","750","750","","1,150"]
["","","","Depth","mm","620","620","","620"]
["","","","Height","mm","200","200","","200"]
["Teža","Unit","","","kg","21","21","","28"]
["Ventilator","Zunanji statični tlak","","Nom.","Pa","30","30","","40"]
["","Hitrost pretoka zraka","Ogrevanje","Visok","m³/min","8.7","8.7","","16.0"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Nizko","m³/min","7.3","7.3","","13.5"]
["","","Hlajenje","Nizko","m³/min","7.3","7.3","","13.5"]
["","","","Medium","m³/min","8.0","8.0","","14.8"]
["","","","Visok","m³/min","8.7","8.7","","16.0"]
["Power supply","Faza","","","","1~","1~","","1~"]
["","Frekvenca","","","Hz","50","50","","50"]
["","Napetost","","","V","220-240","220-240","","220-240"]
["Opombe","","","","","(1) - Glejte ločeno risbo za električne podatke","(1) - Glejte ločeno risbo za električne podatke","","(1) - Glejte ločeno risbo za električne podatke"]
["Vhodna moč","Hlajenje","","Nom.","kW","","","0.060"]
["","Gretje","","Nom.","kW","","","0.060"]
["Mere","Enota","","Višina","mm","","","200"]
["","","","Širina","mm","","","1150"]
["","","","Globina","mm","","","620"]
["Teža","Enota","","","kg","","","28"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","","","15.8"]
["","","","Srednja","m³/min","","","14.6"]
["","","","Nizko","m³/min","","","13.3"]
["","","Gretje","Visok","m³/min","","","15.8"]
["","","Ogrevanje","Srednja","m³/min","","","14.6"]
["","","Gretje","Nizko","m³/min","","","13.3"]
["","Zunanji statični tlak","","Nom.","Pa","","","40"]
["Raven zvočne moči","Hlajenje","","","dBA","","","55.0"]
["","Gretje","","","dBA","","","55.0"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","","38.0"]
["","","","Srednja","dBA","","","35.0"]
["","","","Nizko","dBA","","","30.0"]
["","Gretje","","Visok","dBA","","","38.0"]
["","Ogrevanje","","Srednja","dBA","","","35.0"]
["","Gretje","","Nizko","dBA","","","30.0"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","","6.35"]
["","Plin","","Zun. premer","mm","","","12.70"]
["","Izpust","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standardni pripomočki","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Zračni filter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Napajanje","Faza","","","","","","1~"]
["","Frekvenca","","","Hz","","","50"]
["","Napetost","","","V","","","220-240"]