{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":7,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB / RXS25K3V1B","FDXS35F2VEB / RXS35K2V1B","FDXS50F2VEB / RXS50K2V1B"]
["Hladilna kapaciteta","Min.","","kW","1.3","1.4","1.7"]
["","Maks.","","kW","3.0","3.8","5.3"]
["","Nom.","","kW","2.4 (2)","3.4 (2)","5.0 (2)"]
["Priključki cevne napeljave","Tekočina","Zun. premer","mm","6.35","6.35","6.35"]
["","Plin","Zun. premer","mm","9.5","9.5","12.7"]
["","Drain","OD","mm","VP20 (Zunanji premer 26, Notranji premer 20)","VP20 (Zunanji premer 26, Notranji premer 20)","VP20 (Zunanji premer 26, Notranji premer 20)"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","323","530","825"]
["","EER","","","3.72 (1)","3.21 (1)","3.03 (1)"]
["","COP","","","3.90 (1)","3.39 (1)","3.10 (1)"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","B"]
["","","Ogrevanje","","A","C","D"]
["Grelna kapaciteta","Nom.","","kW","3.2 (3)","4.0 (3)","5.8 (3)"]
["","Min.","","kW","1.3","1.4","1.7"]
["","Maks.","","kW","4.5","5.0","6.0"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(2) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(2) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["","","","","(3) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(3) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(3) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m"]
["","","","","(4) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(4) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(4) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]