{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Raven zvočnega tlaka","Gretje","Visok","dBA","38"]
["","","Srednja","dBA","36"]
["","","Nizko","dBA","30"]
["","Hlajenje","Srednja","dBA","36"]
["","","Nizko","dBA","30"]
["","","Visok","dBA","38"]
["Standardni pripomočki","Priročnik za namestitev","","","1"]
["","Priročnik za upravljanje","","","1"]
["","Izolacija za priključke","","","1"]
["","Tesnilna plošča","","","1"]
["","Objemka, kovinska","","","1"]
["","Cev izpusta","","","1"]
["","Podložka za konzolo obešalnika","","","8"]
["","Tesnilni material","","","2"]
["","Objemke","","","6"]
["","Pritrdilna plošča podložke","","","4"]
["","Vijaki za prirobnice kanala","","","1"]
["","Zračni filter","","","1"]
["Piping connections","Tekočina","Zun. premer","mm","6.35"]
["","Plin","OD","mm","12.7"]
["","priključka","","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Hlajenje","Nom.","kW","0.060"]
["","Gretje","Nom.","kW","0.060"]
["Raven zvočne moči","Hlajenje","","dBA","55"]
["","Gretje","","dBA","55"]
["Mere","Enota","Width","mm","1,150"]
["","","Depth","mm","620"]
["","","Višina","mm","200"]
["Teža","Enota","","kg","30.0"]
["Ventilator","Zunanji statični tlak","Nom.","Pa","40"]
["Power supply","Faza","","","1~"]
["","Frekvenca","","Hz","50/60"]
["","Ime","","","VE"]
["","Napetost","","V","220-240"]
["Opombe","","","","(1) - Ob priklopu na večsistemsko zunanjo enoto glejte specifikacije za multi zunanjo enoto, ki naj se priklopi."]