{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXS-L"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXS50L2V1B","FFA60A2VEB / RXS60L2V1B"]
["Hladilna kapaciteta","Nom.","","kW","5.00","5.70"]
["Hlajenje prostora","SEER","","","5.93","5.71"]
["","Letna poraba energije","","kWh/a","295","349"]
["","Zmogljivost","Pdizajn","kW","5.00","5.70"]
["","Razred energijske učinkovitosti","","","A+","A+"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","3.84","3.96"]
["","SCOP/A","","","3.90","4.04"]
["","Razred energijske učinkovitosti","","","A","A+"]
["","Letna poraba energije","","kWh/a","1,378","1,373"]
["Piping connections","Tekočina","Zun. premer","mm","6.35","6.35"]
["","Plin","Zun. premer","mm","12.70","12.70"]
["","Drain","OD","mm","VP20 (Zunanji premer 26, Notranji premer 20)","VP20 (Zunanji premer 26, Notranji premer 20)"]
["Nazivna učinkovitost","EER","","","3.21","3.02"]
["","Letna por.energ.","","kWh","780","945"]
["","COP","","","3.49","3.41"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","B"]
["","","Ogrevanje","","B","B"]
["Grelna kapaciteta","Nom.","","kW","5.80","7.00"]
["Opombe","","","","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke"]