{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":11,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RZAG-MY1"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / FFA50A2VEB / RZAG71M7Y1B","FFA35A2VEB / FFA35A2VEB / RZAG71M7Y1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZAG71M7Y1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZAG100M7Y1B","FFA50A2VEB / FFA50A2VEB / RZAG100M7Y1B","FFA50A2VEB / FFA50A2VEB / FFA50A2VEB / RZAG100M7Y1B","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZAG100M7Y1B (Archived)"]
["Hladilna kapaciteta","Nom.","","kW","6.80 (1)","","","9.50 (1)","9.50 (1)","9.50 (1)"]
["Hlajenje prostora","SEER","","","7.31","","","8.23","7.03","7.56"]
["","Letna poraba energije","","kWh/a","326","","","404","473","440"]
["","Zmogljivost","Pdizajn","kW","6.80","","","9.50","9.50","9.50"]
["","Razred energijske učinkovitosti","","","A++","","","A++","A++","A++"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","4.70","","","7.80","7.80","7.80"]
["","SCOP/A","","","4.18","","","4.34","4.17","4.44"]
["","Razred energijske učinkovitosti","","","A+","","","A+","A+","A+"]
["","Letna poraba energije","","kWh/a","1,574","","","2,516","2,619","2,460"]
["Grelna kapaciteta","Nom.","","kW","7.50 (2)","","","10.8 (2)","10.8 (2)","10.8 (2)"]
["Opombe","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["Outdoor unit","","","","","RZAG71M7Y1B","RZAG71M7Y1B","","","","RZAG100M7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","","6.80 (1)","6.80 (1)","","","","9.50 (1)"]
["Grelna kapaciteta","Nom.","","kW","","7.50 (2)","7.50 (2)","","","","10.8 (2)"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","A++","A++","","","","A++"]
["","Zmogljivost","Pdizajn","kW","","6.80","6.80","","","","9.50"]
["","SEER","","","","7.11","7.17","","","","7.66"]
["","Letna poraba energije","","kWh/a","","335","332","","","","434"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","A+","A+","","","","A+"]
["","Zmogljivost","Pdizajn","kW","","4.70","4.70","","","","7.80"]
["","SCOP/A","","","","4.22","4.03","","","","4.08"]
["","Letna poraba energije","","kWh/a","","1559","1633","","","","2677"]
["Razpon energetske učinkovitosti","","","","","A+++ ~ D","A+++ ~ D","","","","A+++ ~ D"]