{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Ohišje","Material","","","","Galvanizirana jeklena plošča","Galvanizirana jeklena plošča","Galvanizirana jeklena plošča","Galvanizirana jeklena plošča"]
["Mere","Enota","","Višina","mm","260","260","260","260"]
["","","","Širina","mm","575","575","575","575"]
["","","","Globina","mm","575","575","575","575"]
["Teža","Enota","","","kg","16.0","16.0","17.5","17.5"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","9.0","10.0","12.0","14.5"]
["","","","Srednja","m³/min","8.0","8.5","10.0","12.5"]
["","","","Nizko","m³/min","6.5","6.5","7.5","9.5"]
["","","Gretje","Visok","m³/min","9.0","10.0","12.0","14.5"]
["","","Ogrevanje","Srednja","m³/min","8.0","8.5","10.0","12.5"]
["","","Gretje","Nizko","m³/min","6.5","6.5","7.5","9.5"]
["Raven zvočne moči","Hlajenje","","","dBA","48","51","56","60"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","31.0","34.0","39.0","43.0"]
["","","","Srednja","dBA","28.5","30.5","34.0","40.0"]
["","","","Nizko","dBA","25.0","25.0","27.0","32.0"]
["","Gretje","","Visok","dBA","31.0","34.0","39.0","43.0"]
["","Ogrevanje","","Srednja","dBA","28.5","30.5","34.0","40.0"]
["","Gretje","","Nizko","dBA","25.0","25.0","27.0","32.0"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35","6.35","6.35"]
["","Plin","","Zun. premer","mm","9.52","9.52","12.70","12.70"]
["","Izpust","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Okrasna plošča","Model","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Barva","","","","Bela (N9.5)","Bela (N9.5)","Bela (N9.5)","Bela (N9.5)"]
["","Mere","","Višina","mm","46","46","46","46"]
["","","","Širina","mm","620","620","620","620"]
["","","","Globina","mm","620","620","620","620"]
["","Teža","","","kg","2.8","2.8","2.8","2.8"]
["Okrasna plošča 2","Model","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Barva","","","","Srebrna","Srebrna","Srebrna","Srebrna"]
["","Mere","","Višina","mm","46","46","46","46"]
["","","","Širina","mm","620","620","620","620"]
["","","","Globina","mm","620","620","620","620"]
["","Teža","","","kg","2.8","2.8","2.8","2.8"]
["Okrasna plošča 3","Model","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Barva","","","","Bela (RAL9010)","Bela (RAL9010)","Bela (RAL9010)","Bela (RAL9010)"]
["","Mere","","Višina","mm","55","55","55","55"]
["","","","Širina","mm","700","700","700","700"]
["","","","Globina","mm","700","700","700","700"]
["","Teža","","","kg","2.7","2.7","2.7","2.7"]
["Okrasna plošča 4","Model","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Barva","","","","Bela (RAL9010)","Bela (RAL9010)","Bela (RAL9010)","Bela (RAL9010)"]
["","Mere","","Višina","mm","55","55","55","55"]
["","","","Širina","mm","700","700","700","700"]
["","","","Globina","mm","700","700","700","700"]
["","Teža","","","kg","2.7","2.7","2.7","2.7"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","BRC7EB530 (standardna plošča), BRC7F530W (bela plošča), BRC7F530S (siva plošča)","BRC7EB530 (standardna plošča), BRC7F530W (bela plošča), BRC7F530S (siva plošča)","BRC7EB530 (standardna plošča), BRC7F530W (bela plošča), BRC7F530S (siva plošča)","BRC7EB530 (standardna plošča), BRC7F530W (bela plošča), BRC7F530S (siva plošča)"]
["","Ožičeni daljinski krmilnik","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standardni pripomočki","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240","220-240"]