{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RXM50N2V1B","FFA60A2VEB9 / RXM60N2V1B"]
["Hladilna kapaciteta","Nom.","","kW","5.00"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","772"]
["","EER","","","3.24"]
["","COP","","","3.49"]
["","Direktiva o energijskih oznakah","Hlajenje","","A"]
["","","Ogrevanje","","A"]
["Grelna kapaciteta","Nom.","","kW","5.80"]
["Opombe","","","","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke"]
["Outdoor unit","","","","","RXM60N2V1B"]
["Hladilna kapaciteta","Nom.","","kW","","5.70"]
["Grelna kapaciteta","Nom.","","kW","","7.00"]
["Nom. učink.","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Letna por.energ.","","kWh","","934"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","","B"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","","B"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","A+"]
["","Zmogljivost","Pdizajn","kW","","5.70"]
["","SEER","","","","5.76"]
["","Letna poraba energije","","kWh/a","","347"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","A+"]
["","Zmogljivost","Pdizajn","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","","3.66"]
["","Letna poraba energije","","kWh/a","","1372"]
["Razpon energetske učinkovitosti","","","","","A+++ ~ D"]