{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFQ-B9V / RXS-K"]
[]
[]
[]
[]
["","","","","FFQ25B9V1B / RXS25K2V1B","FFQ25B9V1B / RXS25K3V1B","FFQ35B9V1B / RXS35K2V1B","FFQ50B9V1B / RXS50K2V1B"]
["Hladilna kapaciteta","Nom.","","kW","2.50 (3)","2.50 (3)","3.4 (3)","4.7 (3)"]
["Priključki cevne napeljave","Tekočina","Zun. premer","mm","","","6.35","6.35"]
["","Plin","Zun. premer","mm","","","9.5","12.7"]
["","Izpust","OD","mm","","","VP20 (Zunanji premer 26, Notranji premer 20)","VP20 (Zunanji premer 26, Notranji premer 20)"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","365","365","650","900"]
["","EER","","","3.43","3.43","2.62","2.61"]
["","COP","","","3.48","3.48","2.81","2.81"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","D","D"]
["","","Ogrevanje","","B","B","D","D"]
["Grelna kapaciteta","Nom.","","kW","3.20 (4)","3.20 (4)","4.5 (4)","5.5 (4)"]
["Opombe","","","","(1) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]
["","","","","(3) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m"]
["","","","","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m"]
["","","","","(5) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]