{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / ARXM-A"]
[]
[]
[]
[]
["","","","","FHA71AVEB99 / ARXM71A5V1B","FHA71AVEB9 / ARXM71A5V1B","FHA71AVEB98 / ARXM71A5V1B"]
["Hladilna kapaciteta","Nom.","","kW","6.8","6.8","6.8"]
["Grelna kapaciteta","Nom.","","kW","7.5","7.5","7.5"]
["Nom. učink.","EER","","","3.56","3.56","3.56"]
["","COP","","","3.6","3.6","3.6"]
["","Letna por.energ.","","kWh","955","955","955"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","A","A","A"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","B","B","B"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A+","A+","A+"]
["","Zmogljivost","Pdizajn","kW","6.8","6.8","6.8"]
["","SEER","","","5.87","5.87","5.87"]
["","Letna poraba energije","","kWh/a","406","406","406"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A","A","A"]
["","Zmogljivost","Pdizajn","kW","4.5","4.5","4.5"]
["","SCOP/A","","","3.8","3.8","3.8"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","4.5","4.5","4.5"]
["","Letna poraba energije","","kWh/a","1659","1659","1659"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Opombe","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke","(4) - Glejte ločeno risbo za električne podatke"]